无法找到列 5。
8/9/2024 5:56:27 PM New project 12 succeeded
8/9/2024 5:56:27 PM Communication(COM1)Connection succeeded
8/9/2024 5:56:44 PM Function code (C00.00 Given frequency) communication error
8/9/2024 5:56:44 PM Function code (C00.01 Output frequency) communication error
8/9/2024 5:56:44 PM Function code (C00.02 Output current) communication error
8/9/2024 5:56:45 PM Function code (C00.03 Input voltage) communication error
8/9/2024 5:56:45 PM Function code (C00.04 Output voltage) communication error
8/9/2024 5:56:45 PM Function code (C00.05 Mechanical speed) communication error
8/9/2024 5:56:46 PM Communication(COM1)Disconnected
8/9/2024 5:56:50 PM Successfully modify the communication parameter configuration
8/9/2024 5:56:50 PM Communication(COM1)Connection succeeded
8/9/2024 5:56:52 PM Function code (C00.00 Given frequency) communication error
8/9/2024 5:56:52 PM Function code (C00.01 Output frequency) communication error
8/9/2024 5:56:52 PM Function code (C00.02 Output current) communication error
8/9/2024 5:56:52 PM Function code (C00.03 Input voltage) communication error
8/9/2024 5:56:52 PM Function code (C00.04 Output voltage) communication error
8/9/2024 5:56:53 PM Function code (C00.05 Mechanical speed) communication error
8/9/2024 5:56:53 PM Function code (C00.06 Given torque) communication error
8/9/2024 5:56:53 PM Function code (C00.07 Output torque) communication error
8/9/2024 5:56:55 PM Function code (C00.08 PID Given amount) communication error
8/9/2024 5:56:55 PM Function code (C00.09 PID Feedback amount) communication error
8/9/2024 5:56:56 PM Function code (C00.10 Output Power) communication error
8/9/2024 5:56:56 PM Function code (C00.11 Bus voltage) communication error
8/9/2024 5:56:56 PM Function code (C00.12 Module temperature1) communication error
8/9/2024 5:56:56 PM Function code (C00.13 Module temperature2) communication error
8/9/2024 5:56:56 PM Function code (C00.14 Input terminal X connected state) communication error
8/9/2024 5:56:57 PM Function code (C00.15 Output terminal Y connected state) communication error
8/9/2024 5:56:57 PM Function code (C00.16 Analog AI1 input value) communication error
8/9/2024 5:56:57 PM Function code (C00.17 Analog AI2 input value) communication error
8/9/2024 5:56:57 PM Function code (C00.18 Keyboard potentiometer) communication error
8/9/2024 5:56:57 PM Function code (C00.19 Pulse signal PUL input value) communication error
8/9/2024 5:56:57 PM Function code (C00.20 Analog output AO1) communication error
8/9/2024 5:56:58 PM Function code (C00.21 Analog output AO2 (extended)) communication error
8/9/2024 5:56:58 PM Function code (C00.22 Counter count value) communication error
8/9/2024 5:56:58 PM Function code (C00.23 Running time of this power-on) communication error
8/9/2024 5:56:58 PM Function code (C00.24 Accumulated running time of this machine) communication error
8/9/2024 5:56:58 PM Function code (C00.25 Inverter power rated power) communication error
8/9/2024 5:56:59 PM Function code (C00.26 Inverter rated voltage) communication error
8/9/2024 5:56:59 PM Function code (C00.27 Inverter rated current) communication error
8/9/2024 5:56:59 PM Function code (C00.28 Software version) communication error
8/9/2024 5:56:59 PM Function code (C00.29 PGFeedback frequency) communication error
8/9/2024 5:56:59 PM Function code (C00.30 Timer ) communication error
8/9/2024 5:57:00 PM Function code (C00.31 PID output ) communication error
8/9/2024 5:57:00 PM Function code (C00.32 Software subversion) communication error
8/9/2024 5:57:00 PM Function code (C00.33 Encoder angle) communication error
8/9/2024 5:57:00 PM Function code (C00.34 Z pulse error) communication error
8/9/2024 5:57:00 PM Function code (C00.35 Z pulse count) communication error
8/9/2024 5:57:00 PM Function code (C00.36 Fault warning code) communication error
8/9/2024 5:57:01 PM Function code (C00.37 Cumulative power consumption (low level)) communication error
8/9/2024 5:57:01 PM Function code (C00.38 Accumulated electricity consumption (high　level)) communication error
8/9/2024 5:57:01 PM Function code (C00.39 Power factor angle) communication error
8/9/2024 5:57:01 PM Function code (C00.40) communication error
8/9/2024 5:57:01 PM Function code (C00.41) communication error
8/9/2024 5:57:02 PM Function code (C00.42) communication error
8/9/2024 5:57:02 PM Function code (C00.43) communication error
8/9/2024 5:57:02 PM Function code (C00.44) communication error
8/9/2024 5:57:02 PM Function code (C00.45) communication error
8/9/2024 5:57:02 PM Function code (C00.46) communication error
8/9/2024 5:57:03 PM Function code (C00.47) communication error
8/9/2024 5:57:03 PM Function code (C00.48) communication error
8/9/2024 5:57:03 PM Function code (C00.49) communication error
8/9/2024 5:57:03 PM Function code (C00.50) communication error
8/9/2024 5:57:03 PM Function code (C00.51) communication error
8/9/2024 5:57:03 PM Function code (C00.52) communication error
8/9/2024 5:57:04 PM Function code (C00.53) communication error
8/9/2024 5:57:04 PM Function code (C00.54) communication error
8/9/2024 5:57:04 PM Function code (C00.55) communication error
8/9/2024 5:57:04 PM Function code (C00.56) communication error
8/9/2024 5:57:04 PM Function code (C00.57) communication error
8/9/2024 5:57:05 PM Function code (C00.58) communication error
8/9/2024 5:57:05 PM Function code (C00.59) communication error
8/9/2024 5:57:05 PM Function code (C00.60) communication error
8/9/2024 5:57:05 PM Function code (C00.61) communication error
8/9/2024 5:57:05 PM Function code (C00.62) communication error
8/9/2024 5:57:06 PM Function code (C00.63) communication error
8/9/2024 5:57:06 PM Function code (C00.00 Given frequency) communication error
8/9/2024 5:57:06 PM Function code (C00.01 Output frequency) communication error
8/9/2024 5:57:06 PM Function code (C00.02 Output current) communication error
8/9/2024 5:57:06 PM Function code (C00.03 Input voltage) communication error
8/9/2024 5:57:06 PM Function code (C00.04 Output voltage) communication error
8/9/2024 5:57:07 PM Function code (C00.05 Mechanical speed) communication error
8/9/2024 5:57:07 PM Function code (C00.06 Given torque) communication error
8/9/2024 5:57:07 PM Function code (C00.07 Output torque) communication error
8/9/2024 5:57:07 PM Function code (C00.08 PID Given amount) communication error
8/9/2024 5:57:07 PM Function code (C00.09 PID Feedback amount) communication error
8/9/2024 5:57:08 PM Function code (C00.10 Output Power) communication error
8/9/2024 5:57:08 PM Function code (C00.11 Bus voltage) communication error
8/9/2024 5:57:08 PM Read function code(C00.12 Module temperature1)：28.7
8/9/2024 5:57:08 PM Read function code(C00.13 Module temperature2)：28.7
8/9/2024 5:57:08 PM Read function code(C00.14 Input terminal X connected state)：00000000
8/9/2024 5:57:08 PM Read function code(C00.15 Output terminal Y connected state)：00000000
8/9/2024 5:57:08 PM Read function code(C00.16 Analog AI1 input value)：0.000
8/9/2024 5:57:08 PM Read function code(C00.17 Analog AI2 input value)：1.051
8/9/2024 5:57:08 PM Read function code(C00.18 Keyboard potentiometer)：0.00
8/9/2024 5:57:08 PM Read function code(C00.19 Pulse signal PUL input value)：0.000
8/9/2024 5:57:08 PM Read function code(C00.20 Analog output AO1)：3.33
8/9/2024 5:57:08 PM Read function code(C00.21 Analog output AO2 (extended))：0.00
8/9/2024 5:57:08 PM Read function code(C00.22 Counter count value)：0
8/9/2024 5:57:08 PM Read function code(C00.23 Running time of this power-on)：0.5
8/9/2024 5:57:08 PM Read function code(C00.24 Accumulated running time of this machine)：0
8/9/2024 5:57:08 PM Read function code(C00.25 Inverter power rated power)：5.5
8/9/2024 5:57:08 PM Read function code(C00.26 Inverter rated voltage)：380
8/9/2024 5:57:08 PM Read function code(C00.27 Inverter rated current)：13.0
8/9/2024 5:57:08 PM Read function code(C00.28 Software version)：64.06
8/9/2024 5:57:08 PM Read function code(C00.29 PGFeedback frequency)：0.00
8/9/2024 5:57:08 PM Read function code(C00.30 Timer )：0
8/9/2024 5:57:08 PM Read function code(C00.31 PID output )：0.00
8/9/2024 5:57:09 PM Read function code(C00.32 Software subversion)：100.03
8/9/2024 5:57:09 PM Read function code(C00.33 Encoder angle)：0.00
8/9/2024 5:57:09 PM Read function code(C00.34 Z pulse error)：0
8/9/2024 5:57:09 PM Read function code(C00.35 Z pulse count)：0
8/9/2024 5:57:09 PM Read function code(C00.36 Fault warning code)：0:No failure
8/9/2024 5:57:09 PM Read function code(C00.37 Cumulative power consumption (low level))：0
8/9/2024 5:57:09 PM Read function code(C00.38 Accumulated electricity consumption (high　level))：0
8/9/2024 5:57:09 PM Read function code(C00.39 Power factor angle)：0.0
8/9/2024 5:57:09 PM Read function code(C00.40)：0
8/9/2024 5:57:09 PM Read function code(C00.41)：64727
8/9/2024 5:57:09 PM Read function code(C00.42)：0
8/9/2024 5:57:09 PM Read function code(C00.43)：0
8/9/2024 5:57:09 PM Read function code(C00.44)：0
8/9/2024 5:57:09 PM Read function code(C00.45)：0
8/9/2024 5:57:09 PM Read function code(C00.46)：0
8/9/2024 5:57:09 PM Read function code(C00.47)：15000
8/9/2024 5:57:09 PM Read function code(C00.48)：15000
8/9/2024 5:57:09 PM Read function code(C00.49)：0
8/9/2024 5:57:09 PM Read function code(C00.50)：0
8/9/2024 5:57:09 PM Read function code(C00.51)：34856
8/9/2024 5:57:11 PM Read function code(C00.00 Given frequency)：150.00
8/9/2024 5:57:11 PM Read function code(C00.01 Output frequency)：0.00
8/9/2024 5:57:11 PM Read function code(C00.02 Output current)：0.0
8/9/2024 5:57:11 PM Read function code(C00.03 Input voltage)：283.7
8/9/2024 5:57:11 PM Read function code(C00.04 Output voltage)：0.0
8/9/2024 5:57:11 PM Read function code(C00.05 Mechanical speed)：0
8/9/2024 5:57:11 PM Read function code(C00.06 Given torque)：130.0
8/9/2024 5:57:11 PM Read function code(C00.07 Output torque)：0.0
8/9/2024 5:57:11 PM Read function code(C00.08 PID Given amount)：0.0
8/9/2024 5:57:11 PM Read function code(C00.09 PID Feedback amount)：0.0
8/9/2024 5:57:11 PM Read function code(C00.10 Output Power)：0.0
8/9/2024 5:57:11 PM Read function code(C00.11 Bus voltage)：400.9
8/9/2024 5:57:11 PM Read function code(C00.12 Module temperature1)：28.7
8/9/2024 5:57:11 PM Read function code(C00.13 Module temperature2)：28.7
8/9/2024 5:57:11 PM Read function code(C00.14 Input terminal X connected state)：00000000
8/9/2024 5:57:11 PM Read function code(C00.15 Output terminal Y connected state)：00000000
8/9/2024 5:57:11 PM Read function code(C00.16 Analog AI1 input value)：0.000
8/9/2024 5:57:11 PM Read function code(C00.17 Analog AI2 input value)：1.056
8/9/2024 5:57:11 PM Read function code(C00.18 Keyboard potentiometer)：0.00
8/9/2024 5:57:11 PM Read function code(C00.19 Pulse signal PUL input value)：0.000
8/9/2024 5:57:11 PM Read function code(C00.20 Analog output AO1)：3.33
8/9/2024 5:57:11 PM Read function code(C00.21 Analog output AO2 (extended))：0.00
8/9/2024 5:57:12 PM Read function code(C00.22 Counter count value)：0
8/9/2024 5:57:12 PM Read function code(C00.23 Running time of this power-on)：0.5
8/9/2024 5:57:12 PM Read function code(C00.24 Accumulated running time of this machine)：0
8/9/2024 5:57:12 PM Read function code(C00.25 Inverter power rated power)：5.5
8/9/2024 5:57:12 PM Read function code(C00.26 Inverter rated voltage)：380
8/9/2024 5:57:12 PM Read function code(C00.27 Inverter rated current)：13.0
8/9/2024 5:57:12 PM Read function code(C00.28 Software version)：64.06
8/9/2024 5:57:12 PM Read function code(C00.29 PGFeedback frequency)：0.00
8/9/2024 5:57:12 PM Read function code(C00.30 Timer )：0
8/9/2024 5:57:12 PM Read function code(C00.31 PID output )：0.00
8/9/2024 5:57:12 PM Read function code(C00.32 Software subversion)：100.03
8/9/2024 5:57:12 PM Read function code(C00.33 Encoder angle)：0.00
8/9/2024 5:57:12 PM Read function code(C00.34 Z pulse error)：0
8/9/2024 5:57:12 PM Read function code(C00.35 Z pulse count)：0
8/9/2024 5:57:12 PM Read function code(C00.36 Fault warning code)：0:No failure
8/9/2024 5:57:12 PM Read function code(C00.37 Cumulative power consumption (low level))：0
8/9/2024 5:57:12 PM Read function code(C00.38 Accumulated electricity consumption (high　level))：0
8/9/2024 5:57:12 PM Read function code(C00.39 Power factor angle)：0.0
8/9/2024 5:57:12 PM Read function code(C00.40)：0
8/9/2024 5:57:12 PM Read function code(C00.41)：64727
8/9/2024 5:57:12 PM Read function code(C00.42)：0
8/9/2024 5:57:12 PM Read function code(C00.43)：0
8/9/2024 5:57:12 PM Read function code(C00.44)：0
8/9/2024 5:57:12 PM Read function code(C00.45)：0
8/9/2024 5:57:12 PM Read function code(C00.46)：0
8/9/2024 5:57:12 PM Read function code(C00.47)：15000
8/9/2024 5:57:12 PM Read function code(C00.48)：15000
8/9/2024 5:57:12 PM Read function code(C00.49)：0
8/9/2024 5:57:12 PM Read function code(C00.50)：0
8/9/2024 5:57:12 PM Read function code(C00.51)：34856
8/9/2024 5:57:12 PM Read function code(C00.52)：0
8/9/2024 5:57:12 PM Read function code(C00.53)：30000
8/9/2024 5:57:12 PM Read function code(C00.54)：30000
8/9/2024 5:57:12 PM Read function code(C00.55)：0
8/9/2024 5:57:12 PM Read function code(C00.56)：0
8/9/2024 5:57:12 PM Read function code(C00.57)：65505
8/9/2024 5:57:12 PM Read function code(C00.58)：27
8/9/2024 5:57:12 PM Read function code(C00.59)：50
8/9/2024 5:57:12 PM Read function code(C00.60)：4013
8/9/2024 5:57:13 PM Read function code(C00.61)：0
8/9/2024 5:57:13 PM Read function code(C00.62)：0
8/9/2024 5:57:13 PM Read function code(C00.63)：33686
8/9/2024 5:59:21 PM New project 123 succeeded
8/9/2024 5:59:21 PM Communication(COM1)Connection succeeded
8/9/2024 5:59:24 PM Read function code(C00.00 Given frequency)：150.00
8/9/2024 5:59:24 PM Read function code(C00.01 Output frequency)：0.00
8/9/2024 5:59:24 PM Read function code(C00.02 Output current)：0.0
8/9/2024 5:59:24 PM Read function code(C00.03 Input voltage)：283.5
8/9/2024 5:59:24 PM Read function code(C00.04 Output voltage)：0.0
8/9/2024 5:59:24 PM Read function code(C00.05 Mechanical speed)：0
8/9/2024 5:59:25 PM Read function code(C00.06 Given torque)：130.0
8/9/2024 5:59:25 PM Read function code(C00.07 Output torque)：0.0
8/9/2024 5:59:25 PM Read function code(C00.08 PID given amount)：0.0
8/9/2024 5:59:25 PM Read function code(C00.09 PID feedback quantity)：0.0
8/9/2024 5:59:25 PM Read function code(C00.10 Output power)：0.0
8/9/2024 5:59:25 PM Read function code(C00.11 Bus voltage)：400.5
8/9/2024 5:59:25 PM Read function code(C00.12 Module temperature 1)：28.7
8/9/2024 5:59:25 PM Read function code(C00.13 Module temperature 2)：28.7
8/9/2024 5:59:25 PM Read function code(C00.14 Input terminal X on state)：00000000
8/9/2024 5:59:25 PM Read function code(C00.15 Output terminal Y on state)：00000000
8/9/2024 5:59:25 PM Read function code(C00.16 Analog AI1 input value)：0.000
8/9/2024 5:59:25 PM Read function code(C00.17 Analog AI2 input value)：1.081
8/9/2024 5:59:25 PM Read function code(C00.18 Keypad potentiometer)：0.00
8/9/2024 5:59:25 PM Read function code(C00.19 Pulse signal PUL input value)：0.000
8/9/2024 5:59:25 PM Read function code(C00.20 Analog output AO1)：3.33
8/9/2024 5:59:25 PM Read function code(C00.21 Analog output AO2)：0.00
8/9/2024 5:59:25 PM Read function code(C00.22 Counter count value)：0
8/9/2024 5:59:25 PM Read function code(C00.23 Running time of this power-up)：0.5
8/9/2024 5:59:25 PM Read function code(C00.24 Accumulated running time of this machine)：0
8/9/2024 5:59:25 PM Read function code(C00.25 Inverter power level)：5.5
8/9/2024 5:59:25 PM Read function code(C00.26 Inverter rated voltage)：380
8/9/2024 5:59:25 PM Read function code(C00.27 Inverter rated current)：13.0
8/9/2024 5:59:25 PM Read function code(C00.28 Software version)：64.06
8/9/2024 5:59:25 PM Read function code(C00.29 PG feedback frequency)：0.00
8/9/2024 5:59:25 PM Read function code(C00.30 Timer)：0
8/9/2024 5:59:25 PM Read function code(C00.31 PID output)：0.00
8/9/2024 5:59:25 PM Read function code(C00.32 Software sub version)：100.03
8/9/2024 5:59:25 PM Read function code(C00.33 Encoder Angle)：0.00
8/9/2024 5:59:25 PM Read function code(C00.34 Z-pulse error)：0
8/9/2024 5:59:25 PM Read function code(C00.35 Z-pulse count)：0
8/9/2024 5:59:25 PM Read function code(C00.36 Fault warning code)：0:No fault
8/9/2024 5:59:25 PM Read function code(C00.37 Accumulated power consumption (low))：0
8/9/2024 5:59:25 PM Read function code(C00.38 Accumulated power consumption (high))：0
8/9/2024 5:59:26 PM Read function code(C00.39 Power factor angle)：0.0
8/9/2024 5:59:26 PM Read function code(C00.40)：0
8/9/2024 5:59:26 PM Read function code(C00.41)：64727
8/9/2024 5:59:26 PM Read function code(C00.42)：0
8/9/2024 5:59:26 PM Read function code(C00.43)：0
8/9/2024 5:59:26 PM Read function code(C00.44)：0
8/9/2024 5:59:26 PM Read function code(C00.45)：0
8/9/2024 5:59:26 PM Read function code(C00.46)：0
8/9/2024 5:59:26 PM Read function code(C00.47)：15000
8/9/2024 5:59:26 PM Read function code(C00.48)：15000
8/9/2024 5:59:26 PM Read function code(C00.49)：0
8/9/2024 5:59:26 PM Read function code(C00.50)：0
8/9/2024 5:59:26 PM Read function code(C00.51)：34856
8/9/2024 5:59:26 PM Read function code(C00.52)：0
8/9/2024 5:59:26 PM Read function code(C00.53)：30000
8/9/2024 5:59:26 PM Read function code(C00.54)：30000
8/9/2024 5:59:26 PM Read function code(C00.55)：0
8/9/2024 5:59:26 PM Read function code(C00.56)：0
8/9/2024 5:59:26 PM Read function code(C00.57)：65525
8/9/2024 5:59:26 PM Read function code(C00.58)：65495
8/9/2024 5:59:26 PM Read function code(C00.59)：65508
8/9/2024 5:59:26 PM Read function code(C00.60)：4001
8/9/2024 5:59:26 PM Read function code(C00.61)：0
8/9/2024 5:59:26 PM Read function code(C00.62)：0
8/9/2024 5:59:26 PM Read function code(C00.63)：33686
8/9/2024 5:59:27 PM Read function code(F27.00 Application type selection)：0: general machine
8/9/2024 5:59:30 PM Read function code(F29.00 Ramp1Type)：0: Line 
8/9/2024 5:59:36 PM Real-time monitoring function has been activated
8/9/2024 5:59:40 PM Send forward operation command successfully
8/9/2024 5:59:44 PM Send deceleration to stop command successfully
8/9/2024 5:59:46 PM Send the reversal operation command successfully
8/9/2024 5:59:48 PM Send deceleration to stop command successfully
8/9/2024 6:00:57 PM New project 12 succeeded
8/9/2024 6:00:58 PM Communication(COM1)Connection succeeded
8/9/2024 6:01:01 PM Read function code(C00.00 Given frequency)：150.00
8/9/2024 6:01:01 PM Read function code(C00.01 Output frequency)：0.00
8/9/2024 6:01:01 PM Read function code(C00.02 Output current)：0.0
8/9/2024 6:01:01 PM Read function code(C00.03 Input voltage)：283.9
8/9/2024 6:01:01 PM Read function code(C00.04 Output voltage)：0.0
8/9/2024 6:01:01 PM Read function code(C00.05 Mechanical speed)：0
8/9/2024 6:01:01 PM Read function code(C00.06 Given torque)：130.0
8/9/2024 6:01:01 PM Read function code(C00.07 Output torque)：0.0
8/9/2024 6:01:01 PM Read function code(C00.08 PID Given amount)：0.0
8/9/2024 6:01:01 PM Read function code(C00.09 PID Feedback amount)：0.0
8/9/2024 6:01:01 PM Read function code(C00.10 Output Power)：0.0
8/9/2024 6:01:01 PM Read function code(C00.11 Bus voltage)：401.3
8/9/2024 6:01:01 PM Read function code(C00.12 Module temperature1)：28.7
8/9/2024 6:01:01 PM Read function code(C00.13 Module temperature2)：28.7
8/9/2024 6:01:01 PM Read function code(C00.14 Input terminal X connected state)：00000000
8/9/2024 6:01:01 PM Read function code(C00.15 Output terminal Y connected state)：00000000
8/9/2024 6:01:01 PM Read function code(C00.16 Analog AI1 input value)：0.000
8/9/2024 6:01:01 PM Read function code(C00.17 Analog AI2 input value)：1.081
8/9/2024 6:01:01 PM Read function code(C00.18 Keyboard potentiometer)：0.00
8/9/2024 6:01:01 PM Read function code(C00.19 Pulse signal PUL input value)：0.000
8/9/2024 6:01:01 PM Read function code(C00.20 Analog output AO1)：3.33
8/9/2024 6:01:01 PM Read function code(C00.21 Analog output AO2 (extended))：0.00
8/9/2024 6:01:01 PM Read function code(C00.22 Counter count value)：0
8/9/2024 6:01:01 PM Read function code(C00.23 Running time of this power-on)：0.5
8/9/2024 6:01:01 PM Read function code(C00.24 Accumulated running time of this machine)：0
8/9/2024 6:01:01 PM Read function code(C00.25 Inverter power rated power)：5.5
8/9/2024 6:01:01 PM Read function code(C00.26 Inverter rated voltage)：380
8/9/2024 6:01:01 PM Read function code(C00.27 Inverter rated current)：13.0
8/9/2024 6:01:01 PM Read function code(C00.28 Software version)：64.06
8/9/2024 6:01:02 PM Read function code(C00.29 PGFeedback frequency)：0.00
8/9/2024 6:01:02 PM Read function code(C00.30 Timer )：0
8/9/2024 6:01:02 PM Read function code(C00.31 PID output )：0.00
8/9/2024 6:01:02 PM Read function code(C00.32 Software subversion)：100.03
8/9/2024 6:01:02 PM Read function code(C00.33 Encoder angle)：0.00
8/9/2024 6:01:02 PM Read function code(C00.34 Z pulse error)：0
8/9/2024 6:01:02 PM Read function code(C00.35 Z pulse count)：0
8/9/2024 6:01:02 PM Read function code(C00.36 Fault warning code)：0:No failure
8/9/2024 6:01:02 PM Read function code(C00.37 Cumulative power consumption (low level))：0
8/9/2024 6:01:02 PM Read function code(C00.38 Accumulated electricity consumption (high　level))：0
8/9/2024 6:01:02 PM Read function code(C00.39 Power factor angle)：0.0
8/9/2024 6:01:02 PM Read function code(C00.40)：0
8/9/2024 6:01:02 PM Read function code(C00.41)：10334
8/9/2024 6:01:02 PM Read function code(C00.42)：0
8/9/2024 6:01:02 PM Read function code(C00.43)：0
8/9/2024 6:01:02 PM Read function code(C00.44)：0
8/9/2024 6:01:02 PM Read function code(C00.45)：0
8/9/2024 6:01:02 PM Read function code(C00.46)：0
8/9/2024 6:01:02 PM Read function code(C00.47)：12378
8/9/2024 6:01:02 PM Read function code(C00.48)：53158
8/9/2024 6:01:02 PM Read function code(C00.49)：0
8/9/2024 6:01:02 PM Read function code(C00.50)：0
8/9/2024 6:01:02 PM Read function code(C00.51)：16837
8/9/2024 6:01:02 PM Read function code(C00.52)：0
8/9/2024 6:01:02 PM Read function code(C00.53)：30000
8/9/2024 6:01:02 PM Read function code(C00.54)：30000
8/9/2024 6:01:02 PM Read function code(C00.55)：0
8/9/2024 6:01:02 PM Read function code(C00.56)：0
8/9/2024 6:01:02 PM Read function code(C00.57)：65505
8/9/2024 6:01:02 PM Read function code(C00.58)：65525
8/9/2024 6:01:02 PM Read function code(C00.59)：65508
8/9/2024 6:01:02 PM Read function code(C00.60)：4007
8/9/2024 6:01:02 PM Read function code(C00.61)：0
8/9/2024 6:01:02 PM Read function code(C00.62)：0
8/9/2024 6:01:02 PM Read function code(C00.63)：17802
8/9/2024 6:01:13 PM Read function code(F01.00 Motor 1 way to control )：0:AM VF control 
8/9/2024 6:01:13 PM Read function code(F01.01 Run command channel)：2:RS485 Communication control
8/9/2024 6:01:13 PM Read function code(F01.02 Frequency given source channel A)：0:Keyboard numbers Given frequency
8/9/2024 6:01:13 PM Read function code(F01.03 Frequency given source channel A gain)：100.0
8/9/2024 6:01:13 PM Read function code(F01.04 Frequency given source channel B)：2:Current/voltage analog quantity AI1 given
8/9/2024 6:01:13 PM Read function code(F01.05 Frequency given source channel B  gain)：100.0
8/9/2024 6:01:13 PM Read function code(F01.06 Frequency channel B reference source)：0:Take the maximum output frequency as the reference source 
8/9/2024 6:01:13 PM Read function code(F01.07 Frequency given source selection)：0:Channel A
8/9/2024 6:01:13 PM Read function code(F01.08 Run command bundle )：0000
8/9/2024 6:01:13 PM Read function code(F01.09 Keyboard numbers  Setting  frequency )：150.00
8/9/2024 6:01:13 PM Read function code(F01.10 Maximum frequency )：450.00
8/9/2024 6:01:13 PM Read function code(F01.11 Upper frequency source selection)：0:Upper limit frequency digital given
8/9/2024 6:01:13 PM Read function code(F01.12 Digital setting of upper limit frequency)：400.00
8/9/2024 6:01:13 PM Read function code(F01.13 Lower limit frequency )：0.00
8/9/2024 6:01:13 PM Read function code(F01.14 Frequency Instruction Resolution)：3:1rpm
8/9/2024 6:01:13 PM Read function code(F01.15 Reserved)：0
8/9/2024 6:01:13 PM Read function code(F01.16 Reserved)：0
8/9/2024 6:01:14 PM Read function code(F01.17 Reserved)：0
8/9/2024 6:01:14 PM Read function code(F01.18 Reserved)：0
8/9/2024 6:01:14 PM Read function code(F01.19 Reserved)：0
8/9/2024 6:01:14 PM Read function code(F01.20 Base frequency of acceleration and deceleration time )：0:Maximum frequency 
8/9/2024 6:01:14 PM Read function code(F01.21 Acceleration time unit)：2:0.01S
8/9/2024 6:01:14 PM Read function code(F01.22 Acceleration time 1)：6.00
8/9/2024 6:01:14 PM Read function code(F01.23 Deceleration time 1)：6.00
8/9/2024 6:01:14 PM Read function code(F01.24 Acceleration time 2)：10.00
8/9/2024 6:01:14 PM Read function code(F01.25 Deceleration time 2)：10.00
8/9/2024 6:01:14 PM Read function code(F01.26 Acceleration time 3)：10.00
8/9/2024 6:01:14 PM Read function code(F01.27 Deceleration time 3)：10.00
8/9/2024 6:01:14 PM Read function code(F01.28 Acceleration time 4)：10.00
8/9/2024 6:01:14 PM Read function code(F01.29 Deceleration time 4)：10.00
8/9/2024 6:01:14 PM Read function code(F01.30 S Curve acceleration and deceleration selection )：1
8/9/2024 6:01:14 PM Read function code(F01.31 Acceleration start S-curve time )：0.20
8/9/2024 6:01:14 PM Read function code(F01.32 Acceleration end S curve time )：0.20
8/9/2024 6:01:14 PM Read function code(F01.33 S-curve time to start deceleration )：0.20
8/9/2024 6:01:14 PM Read function code(F01.34 S-curve time at the end of deceleration)：0.20
8/9/2024 6:01:14 PM Read function code(F01.35 Switching frequency between acceleration time 1 and acceleration time 2 )：0.00
8/9/2024 6:01:14 PM Read function code(F01.36 Reserved)：0
8/9/2024 6:01:14 PM Read function code(F01.37 Reserved)：0
8/9/2024 6:01:14 PM Read function code(F01.38 Reserved)：0
8/9/2024 6:01:14 PM Read function code(F01.39 Reserved)：0
8/9/2024 6:01:14 PM Read function code(F01.40 PWM Carrier frequency )：7.0
8/9/2024 6:01:14 PM Read function code(F01.41 PWM Control mode )：1110
8/9/2024 6:01:14 PM Read function code(F01.42 PWM way to control 1)：9101
8/9/2024 6:01:14 PM Read function code(F01.43 Dead zone compensation gain )：306
8/9/2024 6:01:14 PM Read function code(F01.44 Reserved)：15
8/9/2024 6:01:14 PM Read function code(F01.45 Reserved)：40
8/9/2024 6:01:14 PM Read function code(F01.46 Random carrier depth )：0
8/9/2024 6:01:14 PM Read function code(F01.47 Reserved)：0
8/9/2024 6:01:14 PM Read function code(F01.48 Reserved)：10.00
8/9/2024 6:01:14 PM Read function code(F01.49 Reserved)：0.0
8/9/2024 6:01:20 PM Read function code(F05.00 Multi-function input terminal 1(X1))：1:Forward running 
8/9/2024 6:01:20 PM Read function code(F05.01 Multi-function input terminal 2(X2))：2:Reverse run
8/9/2024 6:01:20 PM Read function code(F05.02 Multi-function input terminal 3(X3))：4:Forward jog
8/9/2024 6:01:20 PM Read function code(F05.03 Multi-function input terminal4(X4))：5:Reverse jog
8/9/2024 6:01:20 PM Read function code(F05.04 Multi-function input terminal5(X5))：6:Free stop 
8/9/2024 6:01:20 PM Read function code(F05.05 Multi-function input terminal6(X6))：0:No function 
8/9/2024 6:01:20 PM Read function code(F05.06 Multi-function input terminal7(X7))：0:No function 
8/9/2024 6:01:20 PM Read function code(F05.07 Multi-function input terminal8(X8))：0:No function 
8/9/2024 6:01:20 PM Read function code(F05.08 Multi-function input terminal9(X9))：0:No function 
8/9/2024 6:01:20 PM Read function code(F05.09 Multi-function input terminal10(X10))：0:No function 
8/9/2024 6:01:20 PM Read function code(F05.10 X1 Effective detection delay )：0.010
8/9/2024 6:01:20 PM Read function code(F05.11 X1 Invalid detection delay )：0.010
8/9/2024 6:01:20 PM Read function code(F05.12 X2 Effective detection delay )：0.010
8/9/2024 6:01:20 PM Read function code(F05.13 X2 Invalid detection delay )：0.010
8/9/2024 6:01:20 PM Read function code(F05.14 X3 Effective detection delay )：0.010
8/9/2024 6:01:20 PM Read function code(F05.15 X3 Invalid detection delay )：0.010
8/9/2024 6:01:20 PM Read function code(F05.16 X4 Effective detection delay )：0.010
8/9/2024 6:01:20 PM Read function code(F05.17 X4 Invalid detection delay )：0.010
8/9/2024 6:01:20 PM Read function code(F05.18 X5 Effective detection delay )：0.010
8/9/2024 6:01:20 PM Read function code(F05.19 X5 Invalid detection delay )：0.010
8/9/2024 6:01:20 PM Read function code(F05.20 Terminal control  operation mode )：0:Two-wire system 1
8/9/2024 6:01:20 PM Read function code(F05.21 Reserved)：0000
8/9/2024 6:01:20 PM Read function code(F05.22 X1～X4 Terminal feature selection )：0000
8/9/2024 6:01:20 PM Read function code(F05.23 X5～X8 Terminal feature selection )：0000
8/9/2024 6:01:20 PM Read function code(F05.24 X9～X10 Terminal feature selection )：0000
8/9/2024 6:01:20 PM Read function code(F05.25 Terminal UP / DW control selection)：0:Frequency power down storage 
8/9/2024 6:01:20 PM Read function code(F05.26 Terminal UP/DW control Frequency increase and decrease rate )：0.50
8/9/2024 6:01:20 PM Read function code(F05.27 Emergency stop  deceleration time )：1.00
8/9/2024 6:01:20 PM Read function code(F05.28 Reserved)：0
8/9/2024 6:01:20 PM Read function code(F05.29 Reserved)：0
8/9/2024 6:01:21 PM Read function code(F05.30 PUL port signal source )：0:X5(Max is 5.000KHz)
8/9/2024 6:01:21 PM Read function code(F05.31 PUL Enter the minimum frequency )：0.000
8/9/2024 6:01:21 PM Read function code(F05.32 PUL Minimum frequency correspondence  Setting )：0.00
8/9/2024 6:01:21 PM Read function code(F05.33 PUL input  Maximum frequency )：5.000
8/9/2024 6:01:21 PM Read function code(F05.34 PUL Maximum frequency  correspond  Setting )：100.00
8/9/2024 6:01:21 PM Read function code(F05.35 PUL Filter time )：0.100
8/9/2024 6:01:21 PM Read function code(F05.36 PUL Cut-off frequency )：0.010
8/9/2024 6:01:21 PM Read function code(F05.37 Reserved)：0
8/9/2024 6:01:21 PM Read function code(F05.38 Reserved)：0
8/9/2024 6:01:21 PM Read function code(F05.39 Reserved)：0
8/9/2024 6:01:21 PM Read function code(F05.40 AI input signal type selection mode)：0:DIP switch 
8/9/2024 6:01:21 PM Read function code(F05.41 AI1 input signal type)：0:Voltage 0~10.00V
8/9/2024 6:01:21 PM Read function code(F05.42 AI2 input signal type)：0:Voltage 0~10.00V
8/9/2024 6:01:21 PM Read function code(F05.43 Analog input curve selection)：0000
8/9/2024 6:01:21 PM Read function code(F05.44 Reserved)：0
8/9/2024 6:01:21 PM Read function code(F05.45 Reserved)：0
8/9/2024 6:01:21 PM Read function code(F05.46 Reserved)：0
8/9/2024 6:01:21 PM Read function code(F05.47 Reserved)：0
8/9/2024 6:01:21 PM Read function code(F05.48 Reserved)：0
8/9/2024 6:01:21 PM Read function code(F05.49 Reserved)：0
8/9/2024 6:01:21 PM Read function code(F05.50 AI1 lower limit)：0.0
8/9/2024 6:01:21 PM Read function code(F05.51 AI1 lower limit corresponding setting)：0.00
8/9/2024 6:01:21 PM Read function code(F05.52 AI1 upper limit)：100.0
8/9/2024 6:01:21 PM Read function code(F05.53 AI1 upper limit corresponding setting)：100.00
8/9/2024 6:01:21 PM Read function code(F05.54 AI1 filter time)：0.100
8/9/2024 6:01:21 PM Read function code(F05.55 AI2 lower limit)：0.0
8/9/2024 6:01:21 PM Read function code(F05.56 AI2 lower limit corresponding setting)：0.00
8/9/2024 6:01:21 PM Read function code(F05.57 AI2 upper limit value)：100.0
8/9/2024 6:01:21 PM Read function code(F05.58 AI2 upper limit corresponding setting)：100.00
8/9/2024 6:01:21 PM Read function code(F05.59 AI2 filter time )：0.100
8/9/2024 6:01:21 PM Read function code(F05.60 Curve 1 lower limit )：0.0
8/9/2024 6:01:21 PM Read function code(F05.61 Curve 1 lower limit corresponding setting)：0.00
8/9/2024 6:01:21 PM Read function code(F05.62 Curve 1 turning point 1 input voltage)：30.0
8/9/2024 6:01:21 PM Read function code(F05.63 Curve 1 turning point 1 correspond setting)：30.00
8/9/2024 6:01:21 PM Read function code(F05.64 Curve 1 turning point 2 input voltage)：60.0
8/9/2024 6:01:21 PM Read function code(F05.65 Curve 1 turning point 2 correspond setting)：60.00
8/9/2024 6:01:21 PM Read function code(F05.66 Curve 1 upper limit value)：100.0
8/9/2024 6:01:22 PM Read function code(F05.67 Curve 1 upper limit corresponding setting)：100.00
8/9/2024 6:01:22 PM Read function code(F05.68 Reserved)：0
8/9/2024 6:01:22 PM Read function code(F05.69 Reserved)：0
8/9/2024 6:01:22 PM Read function code(F05.70 Curve 2 lower limit value)：0.0
8/9/2024 6:01:22 PM Read function code(F05.71 Curve 2 lower limit corresponding setting)：0.00
8/9/2024 6:01:22 PM Read function code(F05.72 Curve 2 turning point 1 input voltage)：30.0
8/9/2024 6:01:22 PM Read function code(F05.73 Curve 2 turning point 1 correspond setting)：30.00
8/9/2024 6:01:22 PM Read function code(F05.74 Curve 2 turning point 2 input voltage)：60.0
8/9/2024 6:01:22 PM Read function code(F05.75 Curve 2 turning point 2 correspond setting)：60.00
8/9/2024 6:01:22 PM Read function code(F05.76 Curve 2 upper limit value)：100.0
8/9/2024 6:01:22 PM Read function code(F05.77 Curve 2 upper limit corresponding setting)：100.00
8/9/2024 6:01:22 PM Read function code(F05.78 Reserved)：0
8/9/2024 6:01:22 PM Read function code(F05.79 Reserved)：0
8/9/2024 6:01:22 PM Read function code(F05.80 AI as digital input terminal feature selection)：0000
8/9/2024 6:01:22 PM Read function code(F05.81 AI1 terminal Feature selection (as X))：0:No function
8/9/2024 6:01:22 PM Read function code(F05.82 AI1 High voltage level  Setting)：70.00
8/9/2024 6:01:22 PM Read function code(F05.83 AI1 Low voltage level  Setting)：30.00
8/9/2024 6:01:22 PM Read function code(F05.84 AI2 terminal  Feature selection (as X))：0:No function
8/9/2024 6:01:22 PM Read function code(F05.85 AI2 High voltage level  Setting )：70.00
8/9/2024 6:01:22 PM Read function code(F05.86 AI2 Low voltage level  Setting)：30.00
8/9/2024 6:01:22 PM Read function code(F05.87 Reserved)：1.00
8/9/2024 6:01:22 PM Read function code(F05.88 Reserved)：2.00
8/9/2024 6:01:22 PM Read function code(F05.89 Reserved)：0
8/9/2024 6:01:26 PM Read function code(F02.00 Motor  type )：0:Asynchronous motor （AM）
8/9/2024 6:01:26 PM Read function code(F02.01 Motor poles)：4
8/9/2024 6:01:26 PM Read function code(F02.02 Motor rated power)：5.5
8/9/2024 6:01:26 PM Read function code(F02.03 Motor rated frequency )：50.00
8/9/2024 6:01:26 PM Read function code(F02.04 Motor rated speed)：15000
8/9/2024 6:01:26 PM Read function code(F02.05 Motor rated voltage )：380
8/9/2024 6:01:26 PM Read function code(F02.06 Motor rated current )：13.0
8/9/2024 6:01:26 PM Read function code(F02.07 Motor parameter self tuning selection)：0:No operation 
8/9/2024 6:01:26 PM Read function code(F02.08 Self-learning sign )：0000
8/9/2024 6:01:26 PM Read function code(F02.09 Reserved)：0
8/9/2024 6:01:26 PM Read function code(F02.10 Asynchronous motor  No-load current )：4.9
8/9/2024 6:01:26 PM Read function code(F02.11 Asynchronous motor  Stator resistance )：8080
8/9/2024 6:01:26 PM Read function code(F02.12 Asynchronous motor  Rotor resistance )：5836
8/9/2024 6:01:26 PM Read function code(F02.13 Asynchronous motor  Stator leakage inductance )：537
8/9/2024 6:01:26 PM Read function code(F02.14 Asynchronous motor  Stator inductance)：1356
8/9/2024 6:01:26 PM Read function code(F02.15 Stator resistance per unit value )：4.78
8/9/2024 6:01:26 PM Read function code(F02.16 Rotor resistance per unit value )：3.45
8/9/2024 6:01:26 PM Read function code(F02.17 Stator leakage inductance per unit value)：9.99
8/9/2024 6:01:26 PM Read function code(F02.18 Stator inductance per unit value )：252.4
8/9/2024 6:01:26 PM Read function code(F02.19 Actual value unit selection )：2311
8/9/2024 6:01:26 PM Read function code(F02.20 Synchronous motor stator resistance )：5060
8/9/2024 6:01:26 PM Read function code(F02.21 Synchronous machine d-axis inductance )：5.37
8/9/2024 6:01:26 PM Read function code(F02.22 Synchronous machine q-axis inductance )：5.37
8/9/2024 6:01:26 PM Read function code(F02.23 Synchronous Back EMF)：285
8/9/2024 6:01:26 PM Read function code(F02.24 Synchronous machine encoder installation angle )：0.0
8/9/2024 6:01:26 PM Read function code(F02.25 Synchronous motor Stator resistance per unit value )：2.99
8/9/2024 6:01:27 PM Read function code(F02.26 Synchronous machine d-axis inductance per-unit value )：9.99
8/9/2024 6:01:27 PM Read function code(F02.27 Synchronous machine q-axis inductance per-unit value )：9.99
8/9/2024 6:01:27 PM Read function code(F02.28 Synchronous  Motor Pulse width coefficient)：4050
8/9/2024 6:01:27 PM Read function code(F02.29 Actual value unit selection )：0331
8/9/2024 6:01:27 PM Read function code(F02.30 Speed feedback or encoder type)：0:Ordinary ABZ encoder +AC300PG01 card +EX_B
8/9/2024 6:01:27 PM Read function code(F02.31 Encoder direction)：0:Same direction 
8/9/2024 6:01:27 PM Read function code(F02.32 ABZ encoder Z pulse detection selection)：1:Turn on forward detection
8/9/2024 6:01:27 PM Read function code(F02.33 ABZ Encoder line number )：1024
8/9/2024 6:01:27 PM Read function code(F02.34 Number of poles of resolver )：2
8/9/2024 6:01:27 PM Read function code(F02.35 Encoder transmission ratio numerator )：1
8/9/2024 6:01:27 PM Read function code(F02.36 Encoder transmission ratio denominator )：1
8/9/2024 6:01:27 PM Read function code(F02.37 Encoder speed measurement filter time )：1.0
8/9/2024 6:01:27 PM Read function code(F02.38 Encoder disconnection Check out time )：0.050
8/9/2024 6:01:27 PM Read function code(F02.39 Reserved)：1
8/9/2024 6:01:27 PM Read function code(F02.40 Reserved)：0
8/9/2024 6:01:27 PM Read function code(F02.41 Reserved)：0
8/9/2024 6:01:27 PM Read function code(F02.42 Reserved)：1
8/9/2024 6:01:27 PM Read function code(F02.43 Reserved)：1024
8/9/2024 6:01:27 PM Read function code(F02.44 Reserved)：1.0
8/9/2024 6:01:27 PM Read function code(F02.45 Reserved)：0010
8/9/2024 6:01:27 PM Read function code(F02.46 Reserved)：4
8/9/2024 6:01:27 PM Read function code(F02.47 Z Pulse tolerance)：0
8/9/2024 6:01:27 PM Read function code(F02.48 Z Pulse learning current )：0
8/9/2024 6:01:27 PM Read function code(F02.49 Encoder debug register)：0000
8/9/2024 6:01:27 PM Read function code(F02.50 Motor Online learning function selection)：0:Invalid 
8/9/2024 6:01:27 PM Read function code(F02.51 Stator resistance start learning coefficient 1)：0
8/9/2024 6:01:27 PM Read function code(F02.52 Stator resistance start learning coefficient 2)：0.00
8/9/2024 6:01:27 PM Read function code(F02.53 Stator resistance start learning coefficient 3)：0
8/9/2024 6:01:27 PM Read function code(F02.54 Reserved)：0
8/9/2024 6:01:27 PM Read function code(F02.55 ASR Learning frequency )：60.0
8/9/2024 6:01:27 PM Read function code(F02.56 ASR Learning acceleration and deceleration time )：1.00
8/9/2024 6:01:27 PM Read function code(F02.57 ASR Learning acceleration and deceleration times )：4
8/9/2024 6:01:27 PM Read function code(F02.58 Reserved)：0
8/9/2024 6:01:27 PM Read function code(F02.59 Reserved)：0
8/9/2024 6:01:27 PM Read function code(F02.60 Synchronous motor magnetic pole search function )：0110
8/9/2024 6:01:27 PM Read function code(F02.61 Magnetic pole search current setting value )：0.0
8/9/2024 6:01:28 PM Read function code(F02.62 Magnetic pole search current feedback value )：0.0
8/9/2024 6:01:28 PM Read function code(F02.63 PM Motor inductance learning frequency )：300.00
8/9/2024 6:01:28 PM Read function code(F02.64 PM Motor inductance learning current )：0
8/9/2024 6:01:28 PM Read function code(F02.65 Reserved)：0
8/9/2024 6:01:28 PM Read function code(F02.66 Reserved)：0
8/9/2024 6:01:28 PM Read function code(F02.67 Reserved)：0
8/9/2024 6:01:28 PM Read function code(F02.68 Reserved)：0
8/9/2024 6:01:28 PM Read function code(F02.69 Reserved)：0
8/9/2024 6:01:28 PM Read function code(F02.70 Reserved)：0
8/9/2024 6:01:28 PM Read function code(F02.71 Reserved)：0
8/9/2024 6:01:28 PM Read function code(F02.72 Reserved)：0
8/9/2024 6:01:28 PM Read function code(F02.73 Reserved)：0
8/9/2024 6:01:28 PM Read function code(F02.74 Reserved)：0
8/9/2024 6:01:28 PM Read function code(F02.75 Reserved)：90.0
8/9/2024 6:01:28 PM Read function code(F02.76 Reserved)：0
8/9/2024 6:01:28 PM Read function code(F02.77 Reserved)：0.00
8/9/2024 6:01:28 PM Read function code(F02.78 Reserved)：3
8/9/2024 6:01:28 PM Read function code(F02.79 Reserved)：0
8/9/2024 6:01:28 PM Read function code(F02.80 _LQCoef0)：100.0
8/9/2024 6:01:28 PM Read function code(F02.81)：100.0
8/9/2024 6:01:28 PM Read function code(F02.82)：100.0
8/9/2024 6:01:28 PM Read function code(F02.83)：100.0
8/9/2024 6:01:28 PM Read function code(F02.84)：100.0
8/9/2024 6:01:28 PM Read function code(F02.85)：100.0
8/9/2024 6:01:28 PM Read function code(F02.86)：100.0
8/9/2024 6:01:28 PM Read function code(F02.87)：100.0
8/9/2024 6:01:28 PM Read function code(F02.88)：100.0
8/9/2024 6:01:28 PM Read function code(F02.89)：100.0
8/9/2024 6:01:28 PM Read function code(F02.90)：100.0
8/9/2024 6:01:28 PM Read function code(F02.91)：100.0
8/9/2024 6:01:28 PM Read function code(F02.92)：100.0
8/9/2024 6:01:29 PM Read function code(F02.93)：100.0
8/9/2024 6:01:29 PM Read function code(F02.94)：100.0
8/9/2024 6:01:29 PM Read function code(F02.95)：100.0
8/9/2024 6:01:29 PM Read function code(F02.96)：100.0
8/9/2024 6:01:29 PM Read function code(F02.97)：100.0
8/9/2024 6:01:29 PM Read function code(F02.98)：100.0
8/9/2024 6:01:29 PM Read function code(F02.99)：100.0
8/9/2024 6:01:46 PM New project 31 succeeded
8/9/2024 6:01:46 PM Communication(COM1)Connection succeeded
8/9/2024 6:02:42 PM New project 123 succeeded
8/9/2024 6:02:43 PM Communication(COM1)Connection succeeded
8/9/2024 6:02:52 PM Real-time monitoring function has been activated
8/9/2024 6:02:57 PM Send forward operation command successfully
8/9/2024 6:03:15 PM Read function code(F01.00 Motor 1 control method)：0:AM VF control
8/9/2024 6:03:15 PM Read function code(F01.01 Operation Command Channel)：2:RS485 communication control
8/9/2024 6:03:15 PM Read function code(F01.02 Frequency setting source channel A)：0:Keypad digital frequency setting
8/9/2024 6:03:15 PM Read function code(F01.03 Frequency setting source channel A gain)：100.0
8/9/2024 6:03:15 PM Read function code(F01.04 Frequency setting source channel B)：2:Current/voltage analog AI1 given
8/9/2024 6:03:15 PM Read function code(F01.05 Frequency setting source channel B gain)：100.0
8/9/2024 6:03:15 PM Read function code(F01.06 Frequency channel B reference source)：0:Maximum output frequency as reference source
8/9/2024 6:03:15 PM Read function code(F01.07 Frequency feed source selection)：0:Channel A
8/9/2024 6:03:15 PM Read function code(F01.08 Run Command Bundle)：0000
8/9/2024 6:03:15 PM Read function code(F01.09 Keypad Numeric Setting Frequency)：150.00
8/9/2024 6:03:15 PM Read function code(F01.10 Maximum Frequency)：450.00
8/9/2024 6:03:15 PM Read function code(F01.11 Upper limit frequency source selection)：0:Upper limit frequency digital given
8/9/2024 6:03:15 PM Read function code(F01.12 Upper limit frequency digital setting)：400.00
8/9/2024 6:03:15 PM Read function code(F01.13 Lower limit frequency)：0.00
8/9/2024 6:03:15 PM Read function code(F01.14 Frequency command resolution)：3:1rpm
8/9/2024 6:03:15 PM Read function code(F01.15 Reserved)：0
8/9/2024 6:03:15 PM Read function code(F01.16 Reserved)：0
8/9/2024 6:03:15 PM Read function code(F01.17 Reserved)：0
8/9/2024 6:03:15 PM Read function code(F01.18 Reserved)：0
8/9/2024 6:03:15 PM Read function code(F01.19 Reserved)：0
8/9/2024 6:03:15 PM Read function code(F01.20 Acceleration/deceleration time reference frequency)：0:Maximum frequency
8/9/2024 6:03:15 PM Read function code(F01.21 Acceleration time unit)：2:0.01S
8/9/2024 6:03:16 PM Read function code(F01.22 Acceleration time 1)：6.00
8/9/2024 6:03:16 PM Read function code(F01.23 Deceleration time 1)：6.00
8/9/2024 6:03:16 PM Read function code(F01.24 Acceleration time 2)：10.00
8/9/2024 6:03:16 PM Read function code(F01.25 Deceleration time 2)：10.00
8/9/2024 6:03:16 PM Read function code(F01.26 Acceleration time 3)：10.00
8/9/2024 6:03:16 PM Read function code(F01.27 Deceleration time 3)：10.00
8/9/2024 6:03:16 PM Read function code(F01.28 Acceleration time 4)：10.00
8/9/2024 6:03:16 PM Read function code(F01.29 Deceleration time 4)：10.00
8/9/2024 6:03:16 PM Read function code(F01.30 S-curve acceleration/deceleration selection)：0001
8/9/2024 6:03:16 PM Read function code(F01.31 Acceleration start S-curve time)：0.20
8/9/2024 6:03:16 PM Read function code(F01.32 Acceleration end S-curve time)：0.20
8/9/2024 6:03:16 PM Read function code(F01.33 Deceleration start S-curve time)：0.20
8/9/2024 6:03:16 PM Read function code(F01.34 Deceleration end S-curve time)：0.20
8/9/2024 6:03:16 PM Read function code(F01.35 Acceleration time 1 and acceleration time 2 switching frequency)：0.00
8/9/2024 6:03:16 PM Read function code(F01.36 Reserved)：0
8/9/2024 6:03:16 PM Read function code(F01.37 Reserved)：0
8/9/2024 6:03:16 PM Read function code(F01.38 Reserved)：0
8/9/2024 6:03:16 PM Read function code(F01.39 Reserved)：0
8/9/2024 6:03:16 PM Read function code(F01.40 PWM carrier frequency)：7.0
8/9/2024 6:03:16 PM Read function code(F01.41 PWM control mode)：1110
8/9/2024 6:03:16 PM Read function code(F01.42 PWM control mode 1)：9101
8/9/2024 6:03:16 PM Read function code(F01.43 Deadband compensation gain)：306
8/9/2024 6:03:16 PM Read function code(F01.44 Bootstrap time)：15
8/9/2024 6:03:16 PM Read function code(F01.45 Bootstrap protection time)：40
8/9/2024 6:03:16 PM Read function code(F01.46 Random carrier depth)：0
8/9/2024 6:03:16 PM Read function code(F01.47 Reserved)：0
8/9/2024 6:03:16 PM Read function code(F01.48 Reserved)：10.00
8/9/2024 6:03:16 PM Read function code(F01.49 Reserved)：0.0
8/9/2024 6:08:44 PM New project 21 succeeded
8/9/2024 6:08:45 PM Communication(COM1)Connection succeeded
8/9/2024 6:08:48 PM Read function code(C00.00 Given frequency)：15000
8/9/2024 6:08:48 PM Read function code(C00.01 Output frequency)：500.0
8/9/2024 6:08:48 PM Read function code(C00.02 Output current)：0.0
8/9/2024 6:08:48 PM Read function code(C00.03 Input voltage)：283.7
8/9/2024 6:08:48 PM Read function code(C00.04 Output voltage)：297.5
8/9/2024 6:08:48 PM Read function code(C00.05 Mechanical speed)：15000
8/9/2024 6:08:48 PM Read function code(C00.06 Given torque)：130.0
8/9/2024 6:08:48 PM Read function code(C00.07 Output torque)：0.2
8/9/2024 6:08:48 PM Read function code(C00.08 PID Given amount)：0.0
8/9/2024 6:08:48 PM Read function code(C00.09 PID Feedback amount)：0.0
8/9/2024 6:08:48 PM Read function code(C00.10 Output Power)：0.0
8/9/2024 6:08:48 PM Read function code(C00.11 Bus voltage)：400.3
8/9/2024 6:08:48 PM Read function code(C00.12 Module temperature1)：29.0
8/9/2024 6:08:48 PM Read function code(C00.13 Module temperature2)：29.0
8/9/2024 6:08:48 PM Read function code(C00.14 Input terminal X connected state)：00000000
8/9/2024 6:08:48 PM Read function code(C00.15 Output terminal Y connected state)：10000000
8/9/2024 6:08:48 PM Read function code(C00.16 Analog AI1 input value)：0.000
8/9/2024 6:08:48 PM Read function code(C00.17 Analog AI2 input value)：1.076
8/9/2024 6:08:48 PM Read function code(C00.18 Keyboard potentiometer)：0.00
8/9/2024 6:08:48 PM Read function code(C00.19 Pulse signal PUL input value)：0.000
8/9/2024 6:08:49 PM Read function code(C00.20 Analog output AO1)：3.33
8/9/2024 6:08:49 PM Read function code(C00.21 Analog output AO2 (extended))：3.33
8/9/2024 6:08:49 PM Read function code(C00.22 Counter count value)：0
8/9/2024 6:08:49 PM Read function code(C00.23 Running time of this power-on)：0.6
8/9/2024 6:08:49 PM Read function code(C00.24 Accumulated running time of this machine)：0
8/9/2024 6:08:49 PM Read function code(C00.25 Inverter power rated power)：5.5
8/9/2024 6:08:49 PM Read function code(C00.26 Inverter rated voltage)：380
8/9/2024 6:08:49 PM Read function code(C00.27 Inverter rated current)：13.0
8/9/2024 6:08:49 PM Read function code(C00.28 Software version)：64.06
8/9/2024 6:08:49 PM Read function code(C00.29 PGFeedback frequency)：0
8/9/2024 6:08:49 PM Read function code(C00.30 Timer )：0
8/9/2024 6:08:49 PM Read function code(C00.31 PID output )：0.00
8/9/2024 6:08:49 PM Read function code(C00.32 Software subversion)：100.03
8/9/2024 6:08:49 PM Read function code(C00.33 Encoder angle)：0.00
8/9/2024 6:08:49 PM Read function code(C00.34 Z pulse error)：0
8/9/2024 6:08:49 PM Read function code(C00.35 Z pulse count)：0
8/9/2024 6:08:49 PM Read function code(C00.36 Fault warning code)：0:No failure
8/9/2024 6:08:49 PM Read function code(C00.37 Cumulative power consumption (low level))：0
8/9/2024 6:08:49 PM Read function code(C00.38 Accumulated electricity consumption (high　level))：0
8/9/2024 6:08:49 PM Read function code(C00.39 Power factor angle)：6481.5
8/9/2024 6:08:49 PM Read function code(C00.40)：30
8/9/2024 6:08:49 PM Read function code(C00.41)：59800
8/9/2024 6:08:49 PM Read function code(C00.42)：16
8/9/2024 6:08:49 PM Read function code(C00.43)：43
8/9/2024 6:08:49 PM Read function code(C00.44)：5
8/9/2024 6:08:49 PM Read function code(C00.45)：15000
8/9/2024 6:08:49 PM Read function code(C00.46)：15000
8/9/2024 6:08:49 PM Read function code(C00.47)：15000
8/9/2024 6:08:49 PM Read function code(C00.48)：15000
8/9/2024 6:08:49 PM Read function code(C00.49)：0
8/9/2024 6:08:49 PM Read function code(C00.50)：12842
8/9/2024 6:08:49 PM Read function code(C00.51)：17063
8/9/2024 6:08:49 PM Read function code(C00.52)：12747
8/9/2024 6:08:49 PM Read function code(C00.53)：8571
8/9/2024 6:08:50 PM Read function code(C00.54)：8571
8/9/2024 6:08:50 PM Read function code(C00.55)：10
8/9/2024 6:08:50 PM Read function code(C00.56)：65535
8/9/2024 6:08:50 PM Read function code(C00.57)：10
8/9/2024 6:08:50 PM Read function code(C00.58)：6
8/9/2024 6:08:50 PM Read function code(C00.59)：64
8/9/2024 6:08:50 PM Read function code(C00.60)：4001
8/9/2024 6:08:50 PM Read function code(C00.61)：14999
8/9/2024 6:08:50 PM Read function code(C00.62)：2340
8/9/2024 6:08:50 PM Read function code(C00.63)：44522
8/9/2024 6:08:52 PM Real-time monitoring function has been activated
8/9/2024 6:09:08 PM Read function code(C00.00 Given frequency)：15000
8/9/2024 6:09:08 PM Read function code(C00.01 Output frequency)：500.0
8/9/2024 6:09:08 PM Read function code(C00.02 Output current)：0.0
8/9/2024 6:09:08 PM Read function code(C00.03 Input voltage)：283.7
8/9/2024 6:09:08 PM Read function code(C00.04 Output voltage)：297.5
8/9/2024 6:09:08 PM Read function code(C00.05 Mechanical speed)：15000
8/9/2024 6:09:08 PM Read function code(C00.06 Given torque)：130.0
8/9/2024 6:09:08 PM Read function code(C00.07 Output torque)：0.1
8/9/2024 6:09:08 PM Read function code(C00.08 PID Given amount)：0.0
8/9/2024 6:09:08 PM Read function code(C00.09 PID Feedback amount)：0.0
8/9/2024 6:09:08 PM Read function code(C00.10 Output Power)：0.0
8/9/2024 6:09:08 PM Read function code(C00.11 Bus voltage)：400.3
8/9/2024 6:09:08 PM Read function code(C00.12 Module temperature1)：29.0
8/9/2024 6:09:08 PM Read function code(C00.13 Module temperature2)：29.0
8/9/2024 6:09:08 PM Read function code(C00.14 Input terminal X connected state)：00000000
8/9/2024 6:09:08 PM Read function code(C00.15 Output terminal Y connected state)：10000000
8/9/2024 6:09:08 PM Read function code(C00.16 Analog AI1 input value)：0.000
8/9/2024 6:09:09 PM Read function code(C00.17 Analog AI2 input value)：1.073
8/9/2024 6:09:09 PM Read function code(C00.18 Keyboard potentiometer)：0.00
8/9/2024 6:09:09 PM Read function code(C00.19 Pulse signal PUL input value)：0.000
8/9/2024 6:09:09 PM Read function code(C00.20 Analog output AO1)：3.33
8/9/2024 6:09:09 PM Read function code(C00.21 Analog output AO2 (extended))：3.33
8/9/2024 6:09:09 PM Read function code(C00.22 Counter count value)：0
8/9/2024 6:09:09 PM Read function code(C00.23 Running time of this power-on)：0.6
8/9/2024 6:09:09 PM Read function code(C00.24 Accumulated running time of this machine)：0
8/9/2024 6:09:09 PM Read function code(C00.25 Inverter power rated power)：5.5
8/9/2024 6:09:09 PM Read function code(C00.26 Inverter rated voltage)：380
8/9/2024 6:09:09 PM Read function code(C00.27 Inverter rated current)：13.0
8/9/2024 6:09:09 PM Read function code(C00.28 Software version)：64.06
8/9/2024 6:09:09 PM Read function code(C00.29 PGFeedback frequency)：0
8/9/2024 6:09:09 PM Read function code(C00.30 Timer )：0
8/9/2024 6:09:09 PM Read function code(C00.31 PID output )：0.00
8/9/2024 6:09:09 PM Read function code(C00.32 Software subversion)：100.03
8/9/2024 6:09:09 PM Read function code(C00.33 Encoder angle)：0.00
8/9/2024 6:09:09 PM Read function code(C00.34 Z pulse error)：0
8/9/2024 6:09:09 PM Read function code(C00.35 Z pulse count)：0
8/9/2024 6:09:09 PM Read function code(C00.36 Fault warning code)：0:No failure
8/9/2024 6:09:09 PM Read function code(C00.37 Cumulative power consumption (low level))：0
8/9/2024 6:09:09 PM Read function code(C00.38 Accumulated electricity consumption (high　level))：0
8/9/2024 6:09:09 PM Read function code(C00.39 Power factor angle)：6505.9
8/9/2024 6:09:09 PM Read function code(C00.40)：34
8/9/2024 6:09:09 PM Read function code(C00.41)：11226
8/9/2024 6:09:09 PM Read function code(C00.42)：65522
8/9/2024 6:09:09 PM Read function code(C00.43)：12
8/9/2024 6:09:09 PM Read function code(C00.44)：3
8/9/2024 6:09:09 PM Read function code(C00.45)：15000
8/9/2024 6:09:09 PM Read function code(C00.46)：15000
8/9/2024 6:09:09 PM Read function code(C00.47)：15000
8/9/2024 6:09:09 PM Read function code(C00.48)：15000
8/9/2024 6:09:09 PM Read function code(C00.49)：0
8/9/2024 6:09:09 PM Read function code(C00.50)：12823
8/9/2024 6:09:09 PM Read function code(C00.51)：6917
8/9/2024 6:09:09 PM Read function code(C00.52)：12710
8/9/2024 6:09:09 PM Read function code(C00.53)：0
8/9/2024 6:09:09 PM Read function code(C00.54)：8571
8/9/2024 6:09:09 PM Read function code(C00.55)：65521
8/9/2024 6:09:09 PM Read function code(C00.56)：22
8/9/2024 6:09:10 PM Read function code(C00.57)：37
8/9/2024 6:09:10 PM Read function code(C00.58)：65508
8/9/2024 6:09:10 PM Read function code(C00.59)：65519
8/9/2024 6:09:10 PM Read function code(C00.60)：3990
8/9/2024 6:09:10 PM Read function code(C00.61)：14999
8/9/2024 6:09:10 PM Read function code(C00.62)：2340
8/9/2024 6:09:10 PM Read function code(C00.63)：19725
8/9/2024 6:09:13 PM Read function code(F04.00 Linear VF curve selection )：0:Straight line VF curve 
8/9/2024 6:09:13 PM Read function code(F04.01 Torque increase )：2.5
8/9/2024 6:09:13 PM Read function code(F04.02 Torque boost cut-off frequency )：100.0
8/9/2024 6:09:13 PM Read function code(F04.03 Slip compensation  gain )：0.0
8/9/2024 6:09:13 PM Read function code(F04.04 Slip compensation  limiting )：100.0
8/9/2024 6:09:13 PM Read function code(F04.05 Slip compensation  Filter time )：0.200
8/9/2024 6:09:13 PM Read function code(F04.06 Oscillation suppression gain )：100.0
8/9/2024 6:09:13 PM Read function code(F04.07 Oscillation suppression filter time )：1.0
8/9/2024 6:09:13 PM Read function code(F04.08 Output voltage percentage )：100.0
8/9/2024 6:09:13 PM Read function code(F04.09 Reserved)：0
8/9/2024 6:09:13 PM Read function code(F04.10 Self-set voltage V1)：3.0
8/9/2024 6:09:13 PM Read function code(F04.11 Self-setting frequency F1)：100
8/9/2024 6:09:13 PM Read function code(F04.12 Self-set voltage V2)：28.0
8/9/2024 6:09:13 PM Read function code(F04.13 Self-setting frequency F2)：1000
8/9/2024 6:09:13 PM Read function code(F04.14 Self-set voltage V3)：55.0
8/9/2024 6:09:13 PM Read function code(F04.15 Self-setting frequency F3)：2500
8/9/2024 6:09:13 PM Read function code(F04.16 Self-set voltage V4)：78.0
8/9/2024 6:09:14 PM Read function code(F04.17 Self-setting frequency F4)：3750
8/9/2024 6:09:14 PM Read function code(F04.18 Self-set voltage V5)：100.0
8/9/2024 6:09:14 PM Read function code(F04.19 Self-setting frequency F5)：5000
8/9/2024 6:09:14 PM Read function code(F04.20 V/F Voltage frequency separation  voltage given)：0000
8/9/2024 6:09:14 PM Read function code(F04.21 Voltage frequency separation output voltage digital  Setting )：0.00
8/9/2024 6:09:14 PM Read function code(F04.22 Voltage frequency separation  voltage  acceleration time )：10.00
8/9/2024 6:09:14 PM Read function code(F04.23 Voltage frequency separation  voltage  deceleration time )：10.00
8/9/2024 6:09:14 PM Read function code(F04.24 Voltage-frequency separation shutdown mode)：0:Output voltage、Output frequency Acceleration and deceleration do not affect each other 
8/9/2024 6:09:14 PM Read function code(F04.25 Voltage frequency separation  Setting  voltage )：0.00
8/9/2024 6:09:14 PM Read function code(F04.26 Voltage frequency separation min output voltage)：0
8/9/2024 6:09:14 PM Read function code(F04.27 Reserved)：0
8/9/2024 6:09:14 PM Read function code(F04.28 Reserved)：0
8/9/2024 6:09:14 PM Read function code(F04.29 Reserved)：0
8/9/2024 6:09:14 PM Read function code(F04.30 Automatic energy saving control )：0:Shut down 
8/9/2024 6:09:14 PM Read function code(F04.31 Lower limit of energy saving frequency )：1500
8/9/2024 6:09:14 PM Read function code(F04.32 Energy-saving step-down voltage lower limit )：50.0
8/9/2024 6:09:14 PM Read function code(F04.33 Energy-saving step-down voltage regulation rate )：0.010
8/9/2024 6:09:14 PM Read function code(F04.34 Energy-saving step-down voltage recovery rate )：0.200
8/9/2024 6:09:14 PM Read function code(F04.35 VF Overexcitation gain )：64
8/9/2024 6:09:14 PM Read function code(F04.36 Reserved)：500
8/9/2024 6:09:14 PM Read function code(F04.37 Reserved)：500
8/9/2024 6:09:14 PM Read function code(F04.38 Reserved)：0
8/9/2024 6:09:14 PM Read function code(F04.39 Reserved)：1000
8/9/2024 6:09:14 PM Read function code(F04.40 Reserved)：300
8/9/2024 6:09:14 PM Read function code(F04.41 Reserved)：1000
8/9/2024 6:09:14 PM Read function code(F04.42 Reserved)：1000
8/9/2024 6:09:14 PM Read function code(F04.43 Reserved)：50
8/9/2024 6:09:14 PM Read function code(F04.44 Reserved)：70
8/9/2024 6:09:14 PM Read function code(F04.45 Stabilizer proportional gain )：5.0
8/9/2024 6:09:14 PM Read function code(F04.46 Stabilizer filter coefficient )：0.0
8/9/2024 6:09:14 PM Read function code(F04.47 Stabilizer output limit )：5.0
8/9/2024 6:09:14 PM Read function code(F04.48 Reserved)：5000
8/9/2024 6:09:14 PM Read function code(F04.49 Reserved)：700
8/9/2024 6:09:14 PM Read function code(F04.50 Low-frequency pull-in current )：20.0
8/9/2024 6:09:14 PM Read function code(F04.51 Low frequency pull-in current frequency )：100.0
8/9/2024 6:09:14 PM Read function code(F04.52 High frequency pull current )：10.0
8/9/2024 6:09:14 PM Read function code(F04.53 High frequency pull current  frequency )：10.0
8/9/2024 6:09:14 PM Read function code(F04.54 Reserved)：150
8/9/2024 6:09:15 PM Read function code(F04.55 D Shaft current gain )：0.500
8/9/2024 6:09:15 PM Read function code(F04.56 Q Shaft current gain )：0.800
8/9/2024 6:09:15 PM Read function code(F04.57 D Shaft feedforward gain )：1.000
8/9/2024 6:09:15 PM Read function code(F04.58 Q Shaft feedforward gain )：1.000
8/9/2024 6:09:15 PM Read function code(F04.59 Reserved)：11000
8/9/2024 6:09:15 PM Read function code(F04.60 Flux Control Setting  )：11000
8/9/2024 6:09:15 PM Read function code(F04.61 Flux control proportional gain )：1000
8/9/2024 6:09:15 PM Read function code(F04.62 Flux control integral gain )：200
8/9/2024 6:09:15 PM Read function code(F04.63 Flux controller frequency )：50.0
8/9/2024 6:09:15 PM Read function code(F04.64 Flux controller time )：0.0
8/9/2024 6:09:15 PM Read function code(F04.65 Reserved)：100
8/9/2024 6:09:15 PM Read function code(F04.66 Reserved)：0
8/9/2024 6:09:15 PM Read function code(F04.67 Reserved)：800
8/9/2024 6:09:15 PM Read function code(F04.68 Reserved)：1200
8/9/2024 6:09:15 PM Read function code(F04.69 Reserved)：100
8/9/2024 6:09:20 PM Read function code(C01.00 Fault type)：0
8/9/2024 6:09:20 PM Read function code(C01.01 Faults diagnostic information)：0
8/9/2024 6:09:20 PM Read function code(C01.02 Faults operation frequency)：0
8/9/2024 6:09:20 PM Read function code(C01.03 Faults output voltage)：0.0
8/9/2024 6:09:20 PM Read function code(C01.04 Faults output current)：0.0
8/9/2024 6:09:20 PM Read function code(C01.05 Faults bus voltage)：0.0
8/9/2024 6:09:20 PM Read function code(C01.06 Faults module temperature)：0.0
8/9/2024 6:09:20 PM Read function code(C01.07 Faulty inverter status)：0000
8/9/2024 6:09:20 PM Read function code(C01.08 Fault input terminal status)：00000000
8/9/2024 6:09:20 PM Read function code(C01.09 Fault output terminal status)：00000000
8/9/2024 6:09:20 PM Read function code(C01.10 Last time fault type)：0
8/9/2024 6:09:20 PM Read function code(C01.11 Faults diagnostic information)：0
8/9/2024 6:09:20 PM Read function code(C01.12 Last time fault operation frequency)：0
8/9/2024 6:09:21 PM Read function code(C01.13 Previous failure output voltage)：0.0
8/9/2024 6:09:21 PM Read function code(C01.14 Previous failure output current)：0.0
8/9/2024 6:09:21 PM Read function code(C01.15 Previous failure bus voltage)：0.0
8/9/2024 6:09:21 PM Read function code(C01.16 Previous failure module temperature)：0.0
8/9/2024 6:09:21 PM Read function code(C01.17 Last time faulty inverter status)：0000
8/9/2024 6:09:21 PM Read function code(C01.18 Last time fault input terminal status)：00000000
8/9/2024 6:09:21 PM Read function code(C01.19 Last time fault output terminal status)：00000000
8/9/2024 6:09:21 PM Read function code(C01.20 The first two times fault type)：0
8/9/2024 6:09:21 PM Read function code(C01.21 Faults diagnostic information)：0
8/9/2024 6:09:21 PM Read function code(C01.22 The first three times fault type)：0
8/9/2024 6:09:21 PM Read function code(C01.23 Faults diagnostic information)：0
8/9/2024 6:09:42 PM New project 321 succeeded
8/9/2024 6:09:42 PM Communication(COM1)Connection succeeded
08/13/2024 09:49:28 New project 1234567 succeeded
08/13/2024 09:49:28 Communication()Abnormal connection：The PortName cannot be empty.
Parameter name: PortName
